(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(date "sam. 04 avril 2015")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 100 100)
		(grid_origin 100 100)
		(pcbplotparams
			(layerselection 0x00000000_00000000_00000000_000000a5)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/*D13")
	(net 2 "unconnected-(J1-Pin_10-Pad10)")
	(net 3 "unconnected-(J1-Pin_11-Pad11)")
	(net 4 "GND")
	(net 5 "/~{RESET}")
	(net 6 "VCC")
	(net 7 "/D14{slash}MISO")
	(net 8 "/D15{slash}SCK")
	(net 9 "/D12")
	(net 10 "/*D11")
	(net 11 "/*D10")
	(net 12 "/*D9")
	(net 13 "/D8")
	(net 14 "/D7")
	(net 15 "/*D6")
	(net 16 "/*D5")
	(net 17 "/D4")
	(net 18 "/*D3{slash}SCL")
	(net 19 "+5V")
	(net 20 "/A5")
	(net 21 "/A4")
	(net 22 "/A3")
	(net 23 "/A2")
	(net 24 "/A1")
	(net 25 "/A0")
	(net 26 "/AREF")
	(net 27 "/D2{slash}SDA")
	(net 28 "/D0{slash}RX")
	(net 29 "/D1{slash}TX")
	(net 30 "/D17{slash}SS")
	(net 31 "/D16{slash}MOSI")
	(net 32 "+3V3")
	(footprint "Arduino_MountingHole:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 101.27 83.49)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "MH2"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(embedded_fonts no)
	)
	(footprint "Arduino_MountingHole:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 146.99 98.73)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "MH4"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(embedded_fonts no)
	)
	(footprint "Arduino_MountingHole:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 101.27 98.73)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "MH1"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(embedded_fonts no)
	)
	(footprint "Arduino_MountingHole:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 146.99 83.49)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "MH3"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 103.81 98.73 -90)
		(descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x17 2.54mm single row")
		(property "Reference" "J1"
			(at -2.54 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "Analog"
			(at 2.54 -20.32 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x17, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Arduino_Micro.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -20.32 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/*D13")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/AREF")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/A0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/A1")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/A2")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/A3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/A4")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/A5")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(J1-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(J1-Pin_11-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive+no_connect")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "+5V")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/~{RESET}")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D14{slash}MISO")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/D15{slash}SCK")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 103.81 83.49 -90)
		(descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x17 2.54mm single row")
		(property "Reference" "J2"
			(at 2.54 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "Digital"
			(at -2.794 -20.32 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x17, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Arduino_Micro.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -20.32 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D12")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/*D11")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/*D10")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/*D9")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/D8")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/D7")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/*D6")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/*D5")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/D4")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/*D3{slash}SCL")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/D2{slash}SDA")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/~{RESET}")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/D0{slash}RX")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/D1{slash}TX")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/D17{slash}SS")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/D16{slash}MOSI")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 148.26 82.22)
		(end 100 82.22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100 82.22)
		(end 100 100)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.26 100)
		(end 148.26 82.22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100 100)
		(end 148.26 100)
		(layer "Edge.Cuts")
	)
	(gr_text "ICSP"
		(at 143.18 94.92 0)
		(layer "Dwgs.User")
	)
	(gr_text "USB\nMicro-B"
		(at 102.032 91.11 90)
		(layer "Dwgs.User")
	)
	(embedded_fonts no)
)
