### Navigation

- index
- next |
- previous |
- Mayavi v3.3.0 documentation »
- MLab reference »

Note

This section is only a reference describing the function, please see the chapter on mlab: scripting for 3D plotting for an introduction to mlab and how to interact with and assemble the functions of mlab.

Please see the section on Running mlab scripts for instructions on running the examples.

# Camera handling functions

## move

`enthought.mayavi.mlab.``move`(forward=None, right=None, up=None)
  ::

    Translates the camera and focal point together.

    > The arguments specify the relative distance to translate the camera and focal point, so as to produce the appearence of moving the camera without changing the effective field of view. If called with no arguments, the function returns the absolute position of the camera and focal pointon a cartesian coordinate system.

    > Note that the arguments specify relative motion, although the return value with no arguments is in an absolute coordinate system.

    > Keyword arguments:

    > > forward: | float, optional. The distance in space to translate the camera forward (if positive) or backward (if negative)
    > > right: | float, optional. The distance in space to translate the camera to the right (if positive) or left (if negative)
    > > up: | float, optional. The distance in space to translate the camera up (if positive) or down (if negative)

    > Returns:

    > If no arguments are supplied (or all are None), returns a tuple (camera_position, focal_point_position)

    > otherwise, returns None

    > Examples:

    > Get the current camera position:

    >     >>> cam,foc = move()
    >     >>> cam
    >     array([-0.06317079, -0.52849738, -1.68316389])
    >     >>> foc
    >     array([ 1.25909623,  0.15692708, -0.37576693])

    > Translate the camera:

    >     >>> move(3,-1,-1.2)
    >     >>> move()
    >     (array([ 2.93682921, -1.52849738, -2.88316389]),
    >      array([ 4.25909623, -0.84307292, -1.57576693]))

    > Return to the starting position::

    >       >>> move(-3,1,1.2)
    >       >>> move()
    >       (array([-0.06317079, -0.52849738, -1.68316389]),
    >        array([ 1.25909623,  0.15692708, -0.37576693]))

    > See also :mlab.yaw: yaw the camera (tilt left-right) :mlab.pitch: pitch the camera (tilt up-down) :mlab.roll: control the absolute roll angle of the camera :mlab.view: set the camera position relative to the focal point instead

    > > of in absolute space

## pitch

`enthought.mayavi.mlab.``pitch`(degrees)

  Rotates the camera about the axis corresponding to the “right” direction of the current view. Note that this will change the location of the focal point (although not the camera location).

  This angle is relative to the current direction - the angle is NOT an absolute angle in a fixed coordinate system.

  See also

  Mlab.yaw: | relative rotation about the “up” direction
  Mlab.roll: | absolute roll angle (i.e. “up” direction)
  Mlab.move: | relative translation of the camera and focal point

## roll

`enthought.mayavi.mlab.``roll`(roll=None)

  Sets or returns the absolute roll angle of the camera.

  See also

  Mlab.view: | control the position and direction of the camera

## view

`enthought.mayavi.mlab.``view`(azimuth=None, elevation=None, distance=None, focalpoint=None)

  Sets/Gets the view point for the camera.

  > view(azimuth=None, elevation=None, distance=None, focalpoint=None)

  If called with no arguments this returns the current view of the camera. To understand how this function works imagine the surface of a sphere centered around the visualization. The azimuth argument specifies the the angle “phi” on the x-y plane which varies from 0-360 degrees. The elevation argument specifies the angle “theta” from the z axis and varies from 0-180 degrees. The distance argument is the radius of the sphere and the focalpoint, the center of the sphere.

  Note that if the elevation is close to zero or 180, then the azimuth angle refers to the amount of rotation of a standard x-y plot with respect to the x-axis. Thus, specifying `view(0,0)` will give you a typical x-y plot with x varying from left to right and y from bottom to top.

  Keyword arguments:

  > azimuth: | float, optional. The azimuthal angle (in degrees, 0-360), i.e. the angle subtended by the position vector on a sphere projected on to the x-y plane with the x-axis.
  > elevation: | float, optional. The zenith angle (in degrees, 0-180), i.e. the angle subtended by the position vector and the z-axis.
  > distance: | float, optional. A positive floating point number representing the distance from the focal point to place the camera.
  > focalpoint: | array_like, optional. An array of 3 floating point numbers representing the focal point of the camera.

  Returns:

  If no arguments are supplied it returns a tuple of 4 values `(azimuth, elevation, distance, focalpoint)`, representing the current view. Note that these can be used later on to set the view.

  If arguments are supplied it returns None.

  Examples:

  Get the current view:

       >>> v = view()
       >>> v
      (45.0, 45.0, 25.02794981, array([ 0.01118028,  0.        ,  4.00558996]))

  Set the view in different ways:

      >>> view(45, 45)
      >>> view(240, 120)
      >>> view(distance=20)
      >>> view(focalpoint=(0,0,9))

  Set the view to that saved in v above:

      >>> view(*v)

  See also

  Mlab.roll: | control the roll angle of the camera, ie the direction pointing up

## yaw

`enthought.mayavi.mlab.``yaw`(degrees)

  Rotates the camera about the axis corresponding to the “up” direction of the current view. Note that this will change the location of the focal point (although not the camera location).

  This angle is relative to the current direction - the angle is NOT an absolute angle in a fixed coordinate system.

  See also

  Mlab.pitch: | relative rotation about the “right” direction
  Mlab.roll: | absolute roll angle (i.e. “up” direction)
  Mlab.move: | relative translation of the camera and focal point

### Navigation

- index
- next |
- previous |
- Mayavi v3.3.0 documentation »
- MLab reference »